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Apparatus

Power supply, small lamp, light level meter, metre stick., black cloth

Instructions:
[image: A ruler and a measuring device

AI-generated content may be incorrect.]
 
· Darken the room or minimise the light level and adjust for background light levels.
· Ensure you don’t create shadows over the light meter.  
· Place a black cloth over the bench.
· Place the light detector a distance from the lamp.
· Measure the distance from the light detector to the lamp and the intensity of the light at this distance.
· Repeat for different distances between detector and lamp.
· Present your results.

Risk Assessment
· The light bulb may get hot, do not touch it.
· Do an electrical safety check by observing all the wires.
· Be observant to those around you.
· Do not overload the power supply or put too large a voltage across the bulb.
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